17 LED CHASER CIRCUIT (using NE555P + CD4017BE)2 layers high quality PCB  
1.6mm PCB thickness  
Green color PCB  
HASL( with lead ) surface finish  
1oz copper weight  
Fully tested with flying probe test  
Solder mask for top and bottom layers  
No oxidization ever  
Size of the PCB – 100mmx20mm

Easy to solder without any errors.

Part list

1. 5mm LED -17
2. 100ohm resistor – 1
3. 1k resistors – 1
4. 50k preset – 1
5. 2.2uF capacitors – 1
6. NE555P IC – 1
7. 8 pin IC socket – 1
8. CD4017BE – 1
9. 16 pin IC socket – 1