1 LED DARK SENSITIVE CIRCUIT

2 layers high quality PCB  
1.6mm PCB thickness  
Green color PCB  
HASL( with lead ) surface finish  
1oz copper weight  
Fully tested with flying probe test  
Solder mask for top and bottom layers  
No oxidization ever  
Size of the PCB – 22mmx17mm

Easy to solder without any errors.

Part list

1. 5mm LED -1
2. 1k resistor – 2
3. BC547 transistors – 1
4. 100k preset – 1
5. 5537 LDR – 1