**3 led multi vibrator circuit**

2 layers pcb (top and bottom)

1.6mm pcb thickness

Green color pcb

HASL( with lead ) surface finish

1oz copper weight

Fully tested with flying probe test

Solder mask for top and bottom layers

No oxidization ever

Size of the pcb – 33mm x 20mm

**Part list**

1. 5mm led - 3
2. 39k resistors – 3
3. 47uF capacitors – 3
4. C828 transistors – 3