10 LED KNIGHT RIDER CIRCUIT (USING CD4017BE)2 layers high quality PCB  
1.6mm PCB thickness  
Green color PCB  
HASL( with lead ) surface finish  
1oz copper weight  
Fully tested with flying probe test  
Solder mask for top and bottom layers  
No oxidization ever  
Size of the PCB – 100mmx25mm

Easy to solder without any errors.

Part list

1. 5mm LED -10
2. 120ohm resistor – 1
3. 220ohm resistor – 2
4. 1.8K resistors – 1
5. 18K resistors – 1
6. 50K preset – 1
7. 1N4001 diode – 1
8. 2.2uF capacitors – 2
9. 220uF capacitors – 1
10. C828 transistors – 2
11. CD4017BE – 1
12. 16 pin IC socket – 1