**2 led multi vibrator circuit**

2 layers pcb

1.6mm pcb thickness

Green color pcb

HASL( with lead ) surface finish

1oz copper weight

Fully tested with flying probe test

Solder mask for top and bottom layers

No oxidization ever

Size of the pcb – 24mmx20mm

**Part list**

1. 5mm led -2
2. 33k resistors – 2
3. 100uF capacitors – 2
4. 2n2222 transistors – 2